Syntax:
SAVE filename [start] [end]

Saves a file to the SD card. If start
and end are specified, a binary file
with tag #06 will be created with the
memory content from the address range
start-end (included). If start and
end are not specified, the BASIC
program currently loaded in memory
will be created with the
corresponding #F1 tag.
